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SECTION 1: PRODUCT NAME
PRODUCT NAME: Cementing Fluid loss additive 
SECTION 2: HAZARDS IDENTIFICATION
CHARACTERISTICS: Nonflammable and in explosive.
HEALTH HAZARDS: Irritate eye and skin slightly; Cause irritation of the mucosal and upper respiratory tract.
ENVIROMENTAL HAZARDS: Slightly toxic to fish and animal.
SPECIAL ATTENTION: None.
SECTION 3: COMPOSITION/INFORMATION ON INGREDIENTS
	INGREDIENT NAME
	COMPOSITION
	CAS No.

	Copolymer
	  98%      
	40623-75-4

	Water   
	2%
	7732-18-5


SECTION 4: FIRST AID MEASURES
SKIN CONTACT: Put off contaminated clothing, rinse with soapy and clean flowing water.
EYE CONTACT: Raise the eyelid. Rinse it with plenty of clean flowing water and physiological saline. Consult a doctor if irritation occurs.
INGESTION: Drink plenty of water to induce vomiting; If be uncomfortable, consult a doctor please.
INHALATION: Escape to fresh air; If have breathing difficulties, consult a doctor.
SPECIAL ATTENTION: None.
SECTION 5: FIRE-FIGHTING MEASURES
FLAMMABILITY: See section 9(Physical and Chemical Properties).
FIRE FIGHTING MEDIUM: Foam, dry powder, carbon dioxide, water.  
SPECIAL FIRE-FIGHTING EQUIPMENTS: None.
SECTION 6: ACCIDENTAL RELEASE MEASURES
PERSONAL PRECATIONALS: Use personal protective equipment recommended in Section 8 (Exposure Controls/Personal Protection).
SPILL: Collect the most of leakage, clean the site of leakage.
WASTE TREATMENT METHODS: Be properly buried or handled according to local environment requirement.
PACKING TREATMENT METHODS: Transferred to the dumping site for proper disposal.
SECTION 7: HANDLING AND STORAGE
HANDLING: Keep the containers closed when not in use. Do not get in eyes, on skin. Wear proper personal protection.
STORAGE ATTENTION: Stored in a dry cool place, prevented from the sun and rain, kept away from the heat and fire and incompatible materials.
SPECIAL ATTENTION: None.
SECTION 8: ESPOSURE CONTROLS AND PERSONAL PROTECTION
ENGINEERING CONTROL: Provide exhaust ventilation or other engineering controls to keep the airborne concentrations of vapors or particles below their respective threshold limit value.
RESPIRATORY PROTECTION: Wear dusk mask.
SKIN PROTECTION: Wear standard protective clothing and gloves.
EYE PROTECTION: Wear chemical splash goggles.
SPECIAL ATTENTION: Smoking, food and water drinking are all forbidden. 
SECTION 9: PHYSICAL AND CHEMICAL PROPERTIES
COLOR: White or faint yellow.
BULK DENSITY (g/cm3): 0.70±0.20.
PHYSICAL STATE: Powder.
ODOR: Slightly pungent.
WATER SOLUBILITY: Completely soluble in water.
SECTION 10: STABILITY AND REACTIVITY
AVIOD: Open fire, High temperature.
INCOMPATIBLE MATERIAL: Strong oxidizers.
HAZARDOUS DECOMPOSITION PRODUCTS: None.
SECTION 11: TOXICOLOGICAL INFORMATION
INVASIVE ROUTE: Accidental inhalation or ingestion.
HEALTH HAZARD: Careless ingestion has a stimulating effect on the oral cavity and stomach.
SKIN CONTACT: Contact with skin for a long time, slightly induce skin redness.
EYE CONTACT: Induce eye irritant.
INGESTION: Lead to nausea and vomiting.
INHALATION: Lead to cough and prickle.
CARCINOGENICITY: None.
SPECIAL REMIND: None.
SECTION 12: ECOLOGICAL INFORMATION
BIODEGRADABLE: Not available.
ECOTOXICITY: Not available.
SECTION 13: DISPOSAL CONSIDERATIONS
WASTE TREATMENT METHOD: Be properly buried or handled according to local environment requirement.
PACKING TREATMENT METHOD: Transferred to the dumping site for proper disposal.
SECTION 14: TRANSPORT INFORMATION
This product is not included in the dangerous goods transport international regulations (IMDG,IATA,ADR/RID).
PACKAGE        bag
SECTION 15: REGULATORY INFORMATION
The Management Regulations of Dangerous Chemicals Management 
The Practical Detailed Rules and Regulation for Dangerous Chemicals Management
The Classification and mark of Common Chemical Products (GB 13690-2009)
The General Rule of Common Chemical Products (GB15603-1995)
The Technology Conditions for the Packing Marks for Hazardous Cargo (GB 12463 -1990)
SECTION 16: OTHER INFORMATION
RELEASE DATE: 12/18/2014.
REVISION DATE: 03/01/2022.
SUGGEST FOR AND USED RESTRICTIONS: The product is to be used in applications consistent with our product literature. This product is applied to industry only.
